PIN CONNECTION EXP07:

 **OLED Display (0.96", GND, VDD, SCK, SDA):**

* GND -> GND (ESP32)
* VDD -> 3.3V (ESP32)
* SCK -> GPIO 22 (ESP32)
* SDA -> GPIO 21 (ESP32)

 **Joystick (GND, +5V, VRX, VRY, SW):**

* GND -> GND (ESP32)
* +5V -> 5V (ESP32)
* VRX -> GPIO 34 (ESP32) for horizontal movements (X-axis)
* VRY -> GPIO 35 (ESP32) for vertical movements (Y-axis)
* SW -> GPIO 32 (ESP32) for the joystick button (if needed)